{"text_format":"3","workbook":"xls","n_sheets":2,"sheets":["ARK1668ED","Sheet1"],"not_rendered":{"external_links":1,"defined_names":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"ARK1668ED","index":0,"n_rows":145,"n_cols":16,"rows_kept":145,"merged":[[0,1,0,9]],"flags":["formulas_cached_only"]}
[null,"  REV:0.1"]
[null," R&D Department",{"$nulls":4},"Last update: 2025.06.09"]
["Item","Item Name:","Item Description","Value/Volt","Package:","Manufacturer:","Manufacturer Part No:","Location:","Qty:","unit price (RMB)","total Price  (RMB)","Delivery date","Vendor Remarks","Vendor","Vendor address","Vendor address"]
[null,"Resistor","排阻 0402x4","22R(8P4R)*","SMD0402X4",null,null,"RP1,RP2,RP3,RP4,RP5,RP6,RP7,RP8,RP9,RP10",10]
[null,"Resistor","电阻","0R±5%","SMD0402",null,null,"R27,R60,R61,R80,R82,R97,R102,R134,R135,R142,R143,R146,R154,R155,R163,R170,R193,R195,R206,R228,R241,R242,R274,R279, R283,R335,R343,R346,R358,R360,R372,R378,R394,R440,R445",35]
[null,"Resistor","电阻","22R±5%","SMD0402",null,null,"R34,R39,R70,R75,R76,R77,R78,R152,R176,R177,R181,R201,R203,R204,R205,R229,R238,R239,R244,R245,R246,R258,R259,R262, R263,R264,R265,R266,R267,R268,R269,R270,R275,R277,R278, R280,R281,R284,R285,R286,R287,R288,R289,R302,R303,R304, R305,R306,R307,R309,R310,R311,R315,R316,R318,R319,R323, R334,R349,R351,R352,R353,R354,R355,R356,R357,R359,R365, R366,R368,R369,R370,R371,R395,R396,R397,R398,R400,R401, R402,R403,R404,R405,R406,R407,R408,R409,R412,R413,R414, R415,R417,R423,R427,R430,R431,R432,R433,R435,R443,R444",101]
[null,"Resistor","电阻","100R±5%","SMD0402",null,null,"R19,R22,R66,R68,R149,R150,R317,R329,R332,R333,R341,R342, R347,R367,R377,R437",16]
[null,"Resistor","电阻","220R±5%","SMD0402",null,null,"R218",1]
[null,"Resistor","电阻","470R±5%","SMD0402",null,null,"R18,R64,R65,R172,R173,R237,R392",7]
[null,"Resistor","电阻","1K±5%","SMD0402",null,null,"R17,R83,R84,R85,R86,R87,R88,R89,R90,R145,R147,R209,R223, R320,R321,R322,R340,R391",18]
[null,"Resistor","电阻","1.5K±5%","SMD0402",null,null,"R162",1]
[null,"Resistor","电阻","1.8K±5%","SMD0402",null,null,"R410,R411",2]
[null,"Resistor","电阻","4.7K±5%","SMD0402",null,null,"R55,R56,R62,R63,R99,R100,R140,R141,R144,R153,R159,R164, R165,R167,R168,R169,R178,R183,R184,R220,R225,R227,R271, R272,R308,R313,R314,R324,R325,R327,R330,R331,R344,R345, R348,R350,R362,R363,R364,R373,R379,R380,R381,R382,R390, R393",46]
[null,"Resistor","电阻","8.2K±5%","SMD0402",null,null,"R389",1]
[null,"Resistor","电阻","10K±5%","SMD0402",null,null,"R5,R11,R12,R15,R30,R32,R33,R36,R37,R38,R40,R41,R42,R43,R44,R45,R46,R47,R48,R49,R50,R52,R53,R57,R58,R59,R67,R81,R96,R106,R107,R108,R110,R111,R112,R113,R114,R115,R116,R128,R156,R171,R185,R187,R188,R189,R190,R194,R196,R200,R211,R212,R215,R233,R235,R236,R240,R255,R273,R290,R291,R292,R293,R294,R295,R296,R297,R298,R299,R300,R301,R312,R336,R338,R383,R384,R385,R386,R388,R416,R418,R419,R420,R421,R422,R424,R425,R428,R429,R434,R436,R438,R439,R441,R442",95]
[null,"Resistor","电阻","75K±5%","SMD0402",null,null,"R216",1]
[null,"Resistor","电阻","100K±5%","SMD0402",null,null,"R4,R7,R8,R14,R23,R25,R207,R219,R222,R226,R234",11]
[null,"Resistor","电阻","0.1R±1%","SMD0402",null,null,"R9",1]
[null,"Resistor","电阻","18R±1%","SMD0402",null,null,"R247,R248,R249",3]
[null,"Resistor","电阻","68R±1%","SMD0402",null,null,"R250,R251,R252",3]
[null,"Resistor","电阻","100R±1%","SMD0402",null,null,"R51,R54",2]
[null,"Resistor","电阻","240R±1%","SMD0402",null,null,"R93,R94",2]
[null,"Resistor","电阻","1.0K±1%","SMD0402",null,null,"R92,R95",2]
[null,"Resistor","电阻","2.49K±1%","SMD0402",null,null,"R151",1]
[null,"Resistor","电阻","3.0K±1%","SMD0402",null,null,"R337",1]
[null,"Resistor","电阻","12K±1%","SMD0402",null,null,"R210",1]
[null,"Resistor","电阻","30K±1%","SMD0402",null,null,"R6,R10,R26",3]
[null,"Resistor","电阻","33K±1%","SMD0402",null,null,"R375,R426",2]
[null,"Resistor","电阻","107K±1%","SMD0402",null,null,"R208",1]
[null,"Resistor","电阻","110K±1%","SMD0402",null,null,"R28",1]
[null,"Resistor","电阻","133K±1%","SMD0402",null,null,"R21",1]
[null,"Resistor","电阻","160K±1%","SMD0402",null,null,"R3",1]
[null,"Resistor","电阻","200K±1%","SMD0402",null,null,"R16,R24,R29,R339",4]
[null,"Resistor","电阻","300K±1%","SMD0402",null,null,"R13",1]
[null,"Resistor","电阻","402K±1%","SMD0402",null,null,"R20",1]
[null,"Resistor","电阻","1.0M±1%","SMD0402",null,null,"R31,R243,R261",3]
[null,"Resistor","电阻","2.2M±1%","SMD0402",null,null,"R231",1]
[null,"Resistor","电阻","5.1M±1%","SMD0402",null,null,"R35",1]
[null,"Resistor","电阻","0.22R±1%","SMD0805",null,null,"R224",4]
[null,"Resistor","电阻","75R±1%","SMD0805",null,null,"R221,R253,R254,R257,R260",5]
[null,"Resistor","电阻","1.0R±1%","SMD0805",null,null,"R213,R214 ",2]
[null,"可调电阻","2.4X4.0MM","10K±5%","SMD",null,null,"VR2",1]
[null,"Capacitor","电容","5pF/25V±5% NPO","SMD0402",null,null,"C54,C55,C237,C238",4]
[null,"Capacitor","电容","10pF/25V±5% NPO","SMD0402",null,null,"C224,C225,C226,C309,C333",5]
[null,"Capacitor","电容","12pF/25V±5% NPO","SMD0402",null,null,"C9,C169,C172,C173",4]
[null,"Capacitor","电容","15pF/25V±5% NPO","SMD0402",null,null,"C56,C57,C136,C245",4]
[null,"Capacitor","电容","18pF/25V±5% NPO","SMD0402",null,null,"C212,C219,C220,C231,C232,C257,C264",7]
[null,"Capacitor","电容","22pF/25V±5% NPO","SMD0402",null,null,"C18,C34,C40,C47",4]
[null,"Capacitor","电容","27pF/25V±5% NPO","SMD0402",null,null,"C155,C156",2]
[null,"Capacitor","电容","33pF/25V±5% NPO","SMD0402",null,null,"C204,C205",2]
[null,"Capacitor","电容","100pF/25V±5% NPO","SMD0402",null,null,"C87,C88,C89,C90,C91,C92,C93,C94,C256,C269,C282,C284,C299,C304,C318,C319,C320,C321",18]
[null,"Capacitor","电容","470pF/25V±5% NPO","SMD0402",null,null,"C178",1]
[null,"Capacitor","电容","1.0nF/25V±10% X7R","SMD0402",null,null,"C275,C276,C278,C279",4]
[null,"Capacitor","电容","3.3nF/25V±10% X7R","SMD0402",null,null,"C14",1]
[null,"Capacitor","电容","10nF/25V±10% X7R","SMD0402",null,null,"C58,C164,C175",3]
[null,"Capacitor","电容","22nF/25V±10% X7R","SMD0402",null,null,"C206,C221,C222,C223",4]
[null,"Capacitor","电容","0.1uF/25V+80% _20% Y5V","SMD0402",null,null,"C1,C13,C17,C20,C31,C33,C36,C39,C45,C50,C59,C60,C76,C79,C80,C81,C82,C95,C99,C100,C101,C103,C104,C105,C106,C111,C112, C113,C114,C115,C116,C117,C118,C119,C120,C121,C124,C125, C126,C127,C128,C129,C130,C131,C132,C133,C134,C139,C140, C141,C142,C144,C145,C146,C149,C150,C151,C153,C154,C157, C162,C166,C167,C171,C182,C186,C187,C189,C193,C195,C199, C201,C202,C208,C209,C210,C211,C214,C216,C217,C218,C227, C228,C229,C230,C234,C236,C239,C241,C244,C254,C258,C261, C268,C270,C273,C274,C287,C305,C308,C314,C325,C326,C327, C330,C331,C332,C336",108]
[null,"Capacitor","电容","0.22uF/25V+80% _20% Y5V","SMD0402",null,null,"C203",1]
[null,"Capacitor","电容","1uF/16V+80%_20% Y5V","SMD0402",null,null,"C96,C185,C277,C280,C281,C283,C285,C288,C289,C291,C293, C294,C295,C297,C300,C303,C315,C334",18]
[null,"Capacitor","电容","2.2uF/10V+80%_20% Y5V","SMD0603",null,null,"C29,C61,C62,C63,C64,C65,C66,C67,C68,C69,C70,C73,C74,C75, C77,C83,C84,C85,C86,C137,C174,C200,C246,C247,C248,C249, C250,C251,C252,C253,C255,C262,C263,C266,C317",35]
[null,"Capacitor","电容","10uF/10V+80%_20% Y5V","SMD0603",null,null,"C5,C6,C7,C8,C10,C11,C12,C15,C16,C19,C21,C22,C23,C24,C25, C26,C27,C28,C30,C32,C35,C37,C38,C41,C42,C43,C44,C46,C48, C49,C51,C52,C53,C71,C72,C78,C97,C98,C102,C107,C108,C109, C110,C122,C123,C138,C143,C147,C148,C152,C158,C159,C161, C165,C168,C170,C176,C177,C181,C207,C213,C215,C233,C235, C240,C242,C243,C259,C260,C265,C267,C271,C272,C286,C290, C292,C296,C298,C301,C302,C306,C307,C310,C311,C312,C313, C316,C322,C323,C324,C328,C329,C335,C337,C338",95]
[null,"Capacitor","电容","4.7uF/25V+80%_20% Y5V","SMD0805",null,null,"C3,C4,C179,C180,C183,C184,C188,C190,C191,C192,C196,C197, C198",13]
[null,"Capacitor","电容","4.7uF/50V+80%_20% Y5V","SMD1206",null,null,"C194",1]
[null,"Capacitor","电解电容 8X10mm","220uF/25V±20% 105°C","SMD",null,null,"C2",1]
[null,"二极管","硅二极管","IN4004","DO-214AC",null,null,"D1,D11",2]
[null,"二极管","肖特基二极管","SS36","DO-214AC",null,null,"D3,D4,D7,D8,D13",5]
[null,"二极管","肖特基二极管","SS54","SMC",null,null,"D2",1]
[null,"二极管","开关二极管","LL4148","SMD LL34",null,null,"D12",1]
[null,"二极管","开关二极管","BAV99","SOT-23",null,null,"D5,D9",2]
[null,"二极管","TVS二极管","24V 700A","DO-218",null,"SM8S24A","D14",1,{"$nulls":3},"张 13924651464"]
[null,"二极管","稳压二极管","5.1V","SMD LL34",null,null,"D15",1]
[null,"二极管","稳压二极管","6.8V","SMD LL34",null,null,"D10",1]
[null,"二极管","稳压二极管","18V","SMD LL34",null,null,"D6",1]
[null,"二极管","ESD二极管","5V 0.30pF","DFN-2L",null,"TTA0541SB","ED1,ED2,ED3,ED4,ED5,ED6,ED7,ED8,ED9,ED10,ED11,ED12,ED13,ED14,ED15,ED16,ED17,ED18,ED19,ED20,ED21,ED22,ED23,ED24,ED25,ED26,ED27,ED28,ED29,ED30,ED31,ED32,ED33,ED34,ED35,ED36,ED37,ED38,ED39,ED40,ED41,ED42,ED43,ED44,ED45,ED46,ED47,ED48,ED49,ED50",50,{"$nulls":3},"张 13924651464"]
[null,"二极管","发光二极管 普亮","蓝色","SMD0603",null,null,"LED1,LED2,LED3,LED4,LED5",5]
[null,"三级管","NPN三极管","MMBT3904","SOT-23",null,null,"Q4",1]
[null,"三级管","P沟道MOS管","AP3407","SOT-23",null,null,"Q1",1,{"$nulls":3},"吕 13926511001"]
[null,"三级管","N沟道MOS管","AP35RN06K-AU","TO-252",null,null,"Q3",1,{"$nulls":3},"吕 13926511001"]
[null,"三极管","三极管","DTC144TKA","SMT3",null,null,"Q2",1]
[null,"电感","功率屏蔽电感6.0X6.0X4.5MM","4.7uH±20% 6A","SMD ",null,null,"L1,L23,L24,L25,L32",5,{"$nulls":3},"李 18925257676"]
[null,"电感","功率屏蔽电感4.0X4.0X1.8MM","2.2uH±20% 2.0A","SMD ",null,null,"L2,L3,L4,L5,L21",5,{"$nulls":3},"李 18925257676"]
[null,"电感","共模电感","90R100M±25%100mA","SMD1210",null,"JYCM-1210SF-900P-TA","L6,L7,L8,L9,L10,L11,L12,L13,L14,L15,L16,L17,L18,L19,L20",15,{"$nulls":3},"张 13924651464"]
[null,"电感","共模电感","90R100M±25%400mA","SMD2012",null,"JYCM-2012SF-900TA","L30,L31",2,{"$nulls":3},"张 13924651464"]
[null,"电感","共模电感","50R100M±30%230mA","SMD4532",null,"JYCM-4532EL-510TA","L22",1,{"$nulls":3},"张 13924651464"]
[null,"磁珠","EMI磁珠","100M470R","SMD0805",null,null,"L26,L27,L28,L29",4,{"$nulls":3},"张 13924651464"]
[null,"连接器","FPC座 间距0.5mm 卧式后翻盖双面接","40PIN","SMD",null,null,"J3",1]
[null,"连接器","FPC座 间距0.5mm 卧式后翻盖双面接","50PIN","SMD",null,null,"J1",1]
[null,"连接器","间距0.5mm 卧式 掀盖式下接 带锁扣","50PIN","SMD",null,"FPC","J2",1,{"$nulls":3},"郑 15061849829"]
[null,"连接器","FPC座 间距0.5mm 卧式后翻盖双面接","60PIN","SMD",null,null,"J4",1]
[null,"连接器","FPC座 间距0.5mm 卧式后翻盖双面接","6PIN","SMD",null,null,"J5",1]
[null,"连接器","TFT背光插座 卧式","4PIN","SMD",null,null,"J6",1]
[null,"连接器","单排 插针","1PIN","DIP",null,null,"T1,T2,T3,T4,T5",5]
[null,"连接器","间距2.54mm单排 插针 含跳冒","2PIN","DIP",null,null,"JP1,JP2,JP3,JP4,JP5,JP11,JP24,JP27",8]
[null,"连接器","间距2.54mm单排 插针 含跳冒","3PIN","DIP",null,null,"JP6,JP7,JP8,JP9,JP10,JP12,JP13,JP14,JP15,JP16,JP17,JP18,JP19, JP20,JP21,JP22,JP23,JP25,JP26,JP28",20]
[null,"连接器","间距2.54mm双排 插针 2x10","20PIN","DIP",null,null,"CON5",1]
[null,"连接器","间距2.54mm双排 插针 2x20","40PIN","DIP",null,null,"CON1,CON2,CON3,CON4,CON6",6]
[null,"连接器","GPS天线座 立式","5PIN","DIP",null,null,"ANT1",1]
[null,"连接器","RF座 IPEX H1.25MM母座镀金","3PIN","SMD",null,null,"CN1,CN2",2]
[null,"连接器","HDMI TYPE A","19PIN","SMD",null,null,"CN3",1]
[null,"连接器","RJ-45千兆网口座","14PIN","DIP",null,"LPJG4843HENL","LAN1",1]
[null,"连接器","3.5MM耳机座","4PIN","SMD",null,null,"J14,J15,J16",3]
[null,"连接器","RCA座 黄色","4PIN","DIP",null,null,"J7,J8,J9,J10,J11,J12,J13",7]
[null,"连接器","RCA座 白色","4PIN","DIP",null,null,"J17",1]
[null,"连接器","按键 5.2X5.2X1.5MM","4PIN","SMD",null,null,"KEY1,KEY2,KEY3,KEY4,KEY5",5]
[null,"连接器","电源开关 16X10MM","2PIN","DIP",null,null,"SW1,SW2,SW3",3]
[null,"连接器","电源座 ","3PIN","DIP",null,null,"JK1",1]
[null,"连接器","USB座 ","USB 2.0座 A口 4PIN 90度直脚","DIP",null,null,"USB1,USB2,USB3",3]
[null,"MIC","电容式全向麦克风 直径6.0MM","带滤波电容,-42db","DIP",null,null,"MC1,MC2,MC3,MC4,MC5,MC6,MC7,MC8,MC9,MC10",10]
[null,"IC","DC DC","ACP3084","TDFN3X3-10",null,null,"U6",1,{"$nulls":3},"张 13825267144"]
[null,"IC","DC DC","ACP28262-BAA","SOT23-5",null,null,"U2,U4,U5",3,{"$nulls":3},"张 13825267144"]
[null,"IC","DC DC","EUP2998","SOP-16",null,null,"U22",1,{"$nulls":3},"张 13825267144"]
[null,"IC","DC DC","ACP2728-DAA","SOT23-6",null,null,"U21",1,{"$nulls":3},"张 13825267144"]
[null,"IC","DC DC","ACP2755","SOT23-5",null,null,"U20",1,{"$nulls":3},"张 13825267144"]
[null,"IC","USB电源保护","ACP12522A","SOT23-5",null,null,"U3",1,{"$nulls":3},"张 13825267144"]
[null,"IC","DC DC","EUP3289","SOP-8EP",null,null,"U1",1,{"$nulls":3},"张 13825267144"]
[null,"IC","串口转换","FT232","SSOP-28",null,null,"U17",1]
[null,"IC","1000M PHY","RTL8211FDI-CG","QFN-40",null,null,"U18",1,{"$nulls":3},"林 13684921986"]
[null,"IC","快充","TPS2546","WQFN-16",null,null,"U34",1]
[null,"IC","CAN转换","TJA1042T/3","SOP-8",null,null,"U19",1]
[null,"IC","音频DSP","AK7604VQ","LQFP-48",null,null,"U27",1]
[null,"IC","音频DAC","AK4436","QFN-32",null,null,"U30",1]
[null,"IC","音频ADC","ES7210","QFN-32",null,null,"U31",1]
[null,"IC","CVBS解码","ARK7116","QFN-40","开阳",null,"U23",1]
[null,"IC","AHD解码","RN6854M","QFN-32",null,null,"U24",1]
[null,"IC","ARM主控","ARK1668ED","HBGA445","开阳",null,"U7",1]
[null,"IC","复位","PST803D293NM(2.93V)","SOT-23",null,null,"U8",1,{"$nulls":3},"李  18925257676"]
[null,"IC","G SENSOR","BMA250E","LGA-12",null,null,"U9",1]
[null,"IC","INAND","KLM8G1GETF-B041","TFBGA153",null,null,"U14",1]
[null,"IC","NAND","W29N02KVSIAF","TSOP48",null,null,"U13",1]
[null,"IC","SPI FLASH","W25Q32JVSSIQ","SO-8",null,null,"U15,U16",2]
[null,"IC","苹果解密","3.0版本","DFN-8",null,null,"U10",1]
[null,"IC","LDO 1.2V","MM3571A12NER","SOT23-5",null,null,"U25,U37",2,{"$nulls":3},"李 18925257676"]
[null,"IC","LDO 3.3V","MM3571A33NER","SOT23-5",null,null,"U28,U32,U33",3,{"$nulls":3},"李 18925257676"]
[null,"IC","CLASS D AMP","TMS8213E-TR","QFN-20",null,null,"U29",1,{"$nulls":3},"张 13825267144"]
[null,"IC","HDMI OUT","IT66122FN","LQFP-64",null,null,"U36",1,{"$nulls":3},"段 18823466975"]
[null,"MODULE","5G WIFI+BT","GOC-AN440","SMD",null,null,"U26",1,{"$nulls":3},"李 18665911813"]
[null,"MODULE","GPS","AM1612","SMD 1612","开阳",null,"U38",1]
[null,"MODULE","红外接收头","5V","DIP",null,null,"U35",1]
[null,"Crystal","晶振 4PIN 10ppm负载电容18pF ,-40~85°","12.288MHZ","SMD 3225",null,"2.2.3.1228818C1H","Y6",1,{"$nulls":3},"从 13798594765"]
[null,"Crystal","晶振 4PIN 10ppm负载电容9pF ,-40~85°","24MHZ","SMD 3225",null,"2.2.3.2400009C1H","Y1",1,{"$nulls":3},"从 13798594765"]
[null,"Crystal","晶振 4PIN 10ppm负载电容20pF ,-40~85°","25MHZ","SMD 3225",null,"2.2.3.2500020C1H","Y3",1,{"$nulls":3},"从 13798594765"]
[null,"Crystal","晶振 4PIN 10ppm负载电容18pF ,-40~85°","27MHZ","SMD 3225",null,"2.2.3.2700018C1H","Y4,Y5",2,{"$nulls":3},"从 13798594765"]
[null,"Crystal","晶振,32.768KHz,20PPM,12.5PF,-40~85° ","32.768K","SMD 3215",null,"3.C.3.32768C5C1H","Y2",1,{"$nulls":3},"从 13798594765"]
[null,"线材","2.4+5G双频天线 带卡扣",{"$nulls":9},"强 18565804191"]
[null,"PCB","主板 PCB 4层  ","板厚1.6MM"]

{"sheet":"Sheet1","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"hidden":true,"flags":["formulas_cached_only"]}